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	PRODUCT DATA SHEET
Acumur 3100

	Synonyms
	[bookmark: OLE_LINK1][bookmark: OLE_LINK2]Acumur 3100


	Product Grade
	Industrial


	Description 
& Application
	[bookmark: OLE_LINK3][bookmark: OLE_LINK4]Acumur 3100 is the most excellent scale dispersant in all cooling water treatment chemicals.It has good inhibition for dry-type iron oxide and hydrated iron oxide.It is also an excellent dispersant for all-organic cooling water system.Acumur 3100 can also be used as a phosphate or phosphonate corrosion inhibitor stabilizer.Acumur 3100 is applied to the cooling water and boiler water inhibitors; especially for pressurized conditions and contains iron, zinc and phosphate systems.


	Safety Protection
	Week acidity, avoid contact with eye and skin, once contacted, flush with water.


	Specification
	Solid content% : ≥43
Free Monomer%：≤0.5
pH（1% solution）: ≤3.0
Density(20℃) g/cm3 : ≥1.150
Appearance: Light yellow transparent liquid


	Package 
	In 25Kg or 250Kg net plastic drums. Stored in cool and dry place. 


	Shelf Life
	10 Months.
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