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	PRODUCT DATA SHEET
KW-CP 50

	Synonyms
	KW-CP 50 AA-HPA-AMPS Terpolymer

	
	

	Product Grade
	Industrial


	Description 
& Application
	It is the latest sulfosalt copolymers , contains carboxylic acid groups , hydroxyl , sulfo group , and amido four efficiency groups . With amido group , it can improve the medicament’s anti-gelation ability.High tolerance to calcium , excellent scale inhibition ability for calcium carbonate and organic phosphorus acid calcium.Excellent high temperature tolerance and oxidative stability.Efficient dispersity for iron , indium zinc oxide , bedload etc. inorganic matter.Good threshold effect , and coordinate effect. It can be used as scale inhibitor and dispersant in industrial circulating water system, oilfield refill water system and boiler water.


	Safety Protection
	Acidity, avoid contact with eye and skin, once contacted, flush with water.


	Specification
	Solid content (as acid)% : ≥45
Free Monomer %：≤0.5
pH（1% solution）: ≤3.0
Density(20℃) g/cm3 : ≥1.150
Appearance：light yellow transparent liquid


	Package 
	25L or 200L Drum. Stored in cool and dry place. 


	Shelf Life
	1 year.
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