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   常 州 科 益 化 工 有 限 公 司

  CHANGZHOU KOYE CHEMICAL CO.,LTD.
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	PRODUCT DATA SHEET

ATMP.NA4

	Synonyms
	Tetra sodium salt of Amino Trimethylene phosphonic acid

	CAS Number
	20592-85-2

	Einecs Number
	

	UN No.
	

	Molecular Formula
	C3H8NO9P3Na4 

	Molecular weight
	387

	Structural Formula
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	Product Grade
	Industrial



	Description 

& Application
	ATMP Na4 is the neutral sodium salt of ATMP, can prevent the water into scale salts to form scale, especially the formation of calcium carbonate scale. ATMP, Na4 is suitable for circulating cooling water of thermal power plant, refinery, oil field water injection system, reverse osmosis membrane scale inhibitor. ATMP, Na4 for some other additive also has good compatibility. ATMP, Na4 especially suitable for the neutral to acid formula, generating ammonia smell. 

	Safety Protection
	

	Specification
	Active content（as acid）, %;29.4-32.4

Active content（as salt）, %;38.0-42.0
 Iron,(AS Fe2+),Mg/L ;≤35
pH（1% solution）: ;6.5-7.5
Density(20℃) g/cm3 : 1.35 – 1.45
Appearance： Colorless or light yellow transparent liquid


	Package 
	250L Drum, 1000L IBC or Bulk. Stored in cool and dry place. 


	Shelf Life
	10 months
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